

SPS 8 Paging with Integra Series

v.1.0

Diagrama

Descripción generada automáticamente

SPS 8 PAGING WITH INTEGRA SERIES

To connect and setup the WorkPro SPS 8 Paging BlueLine Digital microphone to the WorkPro Integra series of DSP matrices follow the instructions below:

Interfaz de usuario gráfica, Aplicación

Descripción generada automáticamente

Extracting the unmute command is not at all necessary if the SPS 8 is in AUX mode, and also not if the initial state is as follows, as we will unmute with the outgoing output.

Pantalla de un video juego

Descripción generada automáticamente con confianza media

Configure the initial status on the matrix screen, we set the sending value for each of the outputs (Zones), and music is being played in all zones selected.

Interfaz de usuario gráfica, Tabla

Descripción generada automáticamente

Extracting the routing for MIC to OUT1

Captura de pantalla de computadora

Descripción generada automáticamente con confianza media

Setting the message "on Activate"

Interfaz de usuario gráfica, Tabla

Descripción generada automáticamente

Extracting the routing off for MUSIC to OUT1

Captura de pantalla de computadora

Descripción generada automáticamente con confianza media

Music Off on Z1

Now the opposite do "On Deactive" state

Tabla

Descripción generada automáticamente

Extracting the routing off for MIC to OUT1

Captura de pantalla de computadora

Descripción generada automáticamente

Message for MIC off on Z1.

Tabla

Descripción generada automáticamente

Extracting the message for activate MUSIC to OUT1.

Tabla

Descripción generada automáticamente

In case the music is never to be output on a certain output, decrease the amount of send to the minimum (-72db).

